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	DOCUMENT TYPE
Tunnel IQF Packing Record
	STATUS
Release package

	PRODUCT FAMILY
Eye Link Belt
	FILE CODE
JBL-EYE-LINK-TUNNEL-IQF-PACKING-RECORD


PURPOSE
Records dry packing, spare rods, matched components, belt tags, and export-case evidence.
When Buyers Use This File
Export packing
Accessory review
Pre-shipment release
What Buyers Should Send
Old belt photos or a sample section including chain side or edge detail.
Overall width, pitch, wire diameter, rod diameter, and reinforcement details.
Sprocket photos, tooth count, bore, keyway, and drive-shaft notes.
Product type, IQF route, cleaning requirement, and operating temperature.
Engineering Review Focus
Flat support, reinforcement route, and drive-side fit.
Wire, rod, pitch, and tunnel-IQF application compatibility.
Clean weld finish, replacement logic, and packing evidence.
Expected Output From This Pack
Packing checklist
Accessory log
Shipment evidence fields
Release Rule
This document is intended to improve inquiry quality, reduce mismatch risk, and support controlled engineering communication. Final project releases should stay synchronized with the latest confirmed dimensions, wording, inspection evidence, and packing route.
	Public Contact for Engineering Review
JBL Mesh Belt | Jin Bei Li Metal (Suzhou) Co., Ltd.
Website: www.jblmeshbelt.com
Email: info@jblmeshbelt.com
WhatsApp / Phone: +86 138 1487 2506






