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PURPOSE
Confirms perforation layout, side guards, flights, flatness, and cleaning route before production release.
When Buyers Use This File
Plate layout review
Side-guard review
Heavy-load confirmation
What Buyers Should Send
Old belt photos, drawings, or a physical plate sample.
Overall width, rod diameter, rod pitch, chain pitch, and chain-center distance.
Plate thickness, hole diameter, hole layout, side guard height, and flight spacing.
Product load, impact point, temperature, and washing or drying route.
Engineering Review Focus
Plate thickness, hole layout, rod route, and chain fit.
Heavy-load support, side guard geometry, and flight layout.
Flatness control, burr review, and release protection.
Expected Output From This Pack
Checklist fields
Photo request list
Release checkpoints
Release Rule
This document is intended to improve inquiry quality, reduce mismatch risk, and support controlled engineering communication. Final project releases should stay synchronized with the latest confirmed dimensions, wording, inspection evidence, and packing route.
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